DATE :

BUILDER : WISDOM HOMES

ADDRESS :

**FIVE STAR QUALITY ROOFING CERTIFIES THAT THE ITEMS LISTED BELOW HAVE BEEN INSTALLED TO AUSTRALIAN OR MANUFACTURERS STANDARDS**

Roof tiles in accordance with Australian standards as 2049.2002 and as 2050.2002 as well as Boral Roofing Standards and any builder’s instructions.

Sarking in accordance with Australian standards as 4200.2.1994 and Boral Roofing Standard

Sarking is classified low less than 5 flammability index when tested in accordance with 1530.2.1993

Ridge capping in accordance with Australian standards as 2050,2002 and Boral Roofing Standards, ridge lok has been used as a mechanical fixing to all ridge capping.

Compliance with BCA part 3.5

If you require any further assistance, please don’t hesitate to contact the undersigned

Yours sincerely

MARK WALLACE

DIRECTOR