7 December 2018

**SARKING CERTIFICATE – Five Star Quality Roofing**

**PLANT OF MANUFACTURE: THOR BUILDING PRODUCTS**

**DATE OF INSTALLATION: ………**

|  |  |  |
| --- | --- | --- |
| Roof Profile |  | Location |
| e.g. PRESTIGE - TUNGSTEN | Pass | This letter is to certify that sarking fitted to the entire roof area on the above dwelling by Bristile Roofing has a design flammability index of less than 5 when tested in accordance with AS 1530.2: 1993. The installation also conforms to Part 3.5.1 of the Building Code of Australia and the relevant provisions of AS3959:2009 as indicated below.  BAL 12.5 Clause 5.6.2  BAL 19 Clause 6.6.2  BAL 29 Clause 7.6.2  BAL 40 Clause 8.6.2  The sisalation material installed complies with AS/NZ 4200.2.1994.  Yours sincerely,  **Andy Abrahamson**  General Manager |